,Modello##OTHER##,Material main##OTHER##,Descrizione##OTHER##,Cover Material##OTHER##
ED300_INIM_ver01,,<Per categoria>,"Smoke and heat detector that provide exceptionally high sensitivity to all types o fires.
Tri-colour LED.
Integrated short-circuit isolator.
Up to 240 devices connectable to the loop.
Automatic addressing (each device is identified by a factory-assigned serial number).
Supervised remote output configurable from the control panel.
Automatic recognition of remote signaller connection.
Aumatic drift compensation.
Sensitivity selection for smoke (and  0.08 dB/m – 0.10 dB/m – 0.12 dB/m - 0.15dB/m ) and heat (A1R, B, A2S, BR) thresholds 
Operating mode selection: only smoke, only heat, AND mode, OR mode, PLUS mode
Complete diagnostics: view the contamination level in the optical chamber and verify real-time values.
Memory of the smoke and temperature levels measured in the five minutes period prior to the last alarm detected
Vast range of settable options
Bypass plate on the base to give continuity to the line in the event of removal of a detector, possibility to test loop wiring continuity.
Able to auto-drawing installation topology and obtain an easy-to-use, interactive loop layout map
",<Per categoria>
