##### Front Panel (16/24-port)

The following figure uses a 16-port 100 Mbps cloud managed device as an example, and might differ from the actual product.

Figure 1 Front panel (16/24-port)
Table 1 Description of front panel (16/24-port)

No. | Name | Description
--- | --- | ---
1 | PoE ports | 16/24 × 10/100 Mbps or 10/100/1000 Mbps self-adaptive Ethernet ports.
2 | Uplink ports | 10/100/1000 Mbps self-adaptive Ethernet ports and 1000 Mbps optical ports. NOTE The uplink ports are combo ports on select models.
3 | Reset button | Press and hold it for more than 5 seconds, and release after the panel status indicators all turn on to restore the Device to default settings.
4 | Console serial port | Device debugging port. NOTE Only supported by select models.
5 | PoE output power indicator | On: Connected to device. Off: Not connected to device. Flashing: Transmitting data.
6 | Link/Act indicator | On: Connected to the Device. Off: Not connected to the Device. Flashing: Transmitting data.
7 | PoE port status indicators | On: Powered by PoE. Off: Not powered by PoE.
8 | Uplink port status (Link) indicators | On: Connected to device. Off: Not connected to device.
9 | Power indicator | On: Power on. Off: Power off.
10 | System status indicator (SYS) | Flashes: The system works normally.

Related topics

- Front Panel
- Front Panel (4/8-port)