##### Front Panel (4/8-port)

The following figure uses an 8-port 100 Mbps cloud managed device as an example, and might differ from the actual product.

Figure 1 Front panel (4/8-port)
Table 1 Description of front panel (4/8-port)

No. | Name | Description
--- | --- | ---
1 | Reset button | Press and hold it for more than 5 seconds, and release after the panel status indicators all turn on to restore the Device to default settings.
2 | PoE ports | 4/8 × 10/100 Mbps or 10/100/1000 Mbps self-adaptive PoE Ethernet ports.
3 | Uplink ports | 10/100/1000 Mbps self-adaptive Ethernet ports. NOTE The number of the uplink ports might differ from different models. Please refer to the actual product. Some models support 1000 Mbps optical ports. Please refer to the actual product.
4 | Power indicator | On: Power on. Off: Power off.
5 | System status indicator (SYS) | Flashes: The system works normally.
6 | Uplink port status indicators | Link indicator. On: Connected to the Device. Off: Not connected to the Device.
Activity indicator. Flashing: Transmitting data. Off: Not transmitting data.
7 | PoE port status indicators | PoE port status indicator. On: Powered by PoE. Off: Not powered by PoE.
Link/Act indicator | Link/Act indicator. On: Connected to the Device. Off: Not connected to the Device. Flashing: Transmitting data.

Related topics

- Front Panel
- Front Panel (16/24-port)