##### Wall Mount

###### Procedure

1. Drill two M4 screws into the wall, leaving a space of 4 mm between the wall and the head of the screw.
   NOTE
   - Screws do not come with the package. Purchase them as needed.
   - Make sure that the distance between the screws is the distance between the wall-mount holes (77.8 mm for a 4-port switch and 128.4 mm for an 8-port switch).
2. Align the wall-mount holes on the back cover of the Device with the screws, and hang the Device on the screws.
   Figure 1 Wall mount

Related topics

- Installation
- Preparation
- Desktop Mount
- Rack Mount