##### Initializing the Device

###### Prerequisites

- Make sure that the Device is connected to the power supply.
- Make sure that the Device is connected to the computer, and the IP addresses of the computer and the Device are on the same segment.
- Device initialization is required for first-time use or after the Device has been reset.
- Plan the network segment properly to connect the Device to the network.
- By default, DHCP is enabled on the Device. When connected to a network, the Device typically obtains an IP address from a DHCP server, and then you can obtain the IP address of the Device from the upstream device, such as a router. If a DHCP server is not available, the IP address of the Device is 192.168.1.110 by default.
  NOTE

###### Procedure

1. Open the browser, enter the IP address of the Device in the address bar, and then press the Enter key.
2. Select the language and then click Next.
3. Read the legal statement, select I have read and agree to the terms of the Software License Agreement and Privacy Policy, and then click Next.
4. Configure the password.
   - The default username is admin.
   - Configure a high security password according to the prompt of password strength. A password should be 8-32 characters containing at least two types among numbers, letters and common characters (any visible characters other than' " ; : &).
5. Click Complete.

Related topics

- Managing the Device by Local Webpage
- Login the Device