##### Rear Panel (16/24-port)

NOTE

The figures might differ from different models. Please refer to the actual product.

Figure 1 Rear panel (16/24 port)
Table 1 Description of rear panel (16/24 port)

No. | Name | Description
--- | --- | ---
1 | DIP switch | Supported by select models.
2 | Power port | Supports 100–240 VAC.
3 | Ground terminal | Connecting GND. NOTE Normal GND connection of the Device guarantees device lightning protection and anti-interference. You must connect the GND cable before powering on the Device and power off the Device before disconnecting the GND cable. The sectional area of the GND cable must be more than 2.5 mm2, and the GND resistance must be less than 4 Ω.

Related topics

- Rear Panel
- Rear Panel (4/8-port)