##### Connecting Ethernet Port

Ethernet port adopts standard RJ-45 port. With self-adaptation function, it can be automatically configured to full duplex/half-duplex operation mode. It supports MDI/MDI-X self-recognition of the cable, therefore, you can use cross-over cable or straight-through cable to connect terminal device to network device.
Figure 1 Ethernet port pin number
Figure 2 Pin description

The cable connection of RJ-45 connector conforms to the standard 568B (1-orange white, 2-orange, 3-green white, 4-blue, 5-blue white, 6-green, 7-brown white, 8-brown).

Related topics

- Connecting GND Cable
- Connecting Power Cord
- Connecting SFP Ethernet Port
- Connecting PoE Ethernet Port